<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="8.2.2">
<drawing>
<board>
<plain>
<wire x1="39.37" y1="8.89" x2="161.27" y2="8.89" width="0" layer="20"/>
<wire x1="161.27" y1="8.89" x2="161.27" y2="83.49" width="0" layer="20"/>
<wire x1="161.27" y1="83.49" x2="39.37" y2="83.49" width="0" layer="20"/>
<wire x1="39.37" y1="83.49" x2="39.37" y2="8.89" width="0" layer="20"/>
</plain>
<libraries>
<library name="linear">
<description>&lt;b&gt;Linear Devices&lt;/b&gt;&lt;p&gt;
Operational amplifiers,  comparators, voltage regulators, ADCs, DACs, etc.&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="TO220H">
<description>&lt;b&gt;TO-220&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Connectors&lt;/h3&gt;
This library contains electrically-functional connectors. 
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="2X20_SHROUDED">
<description>&lt;h3&gt;Plated Through Hole - 2x20 Shrouded Header&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:40&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;&lt;a href=”https://cdn.sparkfun.com/datasheets/Dev/RaspberryPi/B-D-xx1X.pdf”&gt;Datasheet referenced for footprint&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_20x2&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
</packages>
</library>
<library name="pinhead">
<description>&lt;b&gt;Pin Header Connectors&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="1X02">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
<package name="1X04">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="transistor-power">
<description>&lt;b&gt;Power Transistors&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="TO220BH">
<description>&lt;b&gt;Molded Package&lt;/b&gt;&lt;p&gt;
grid 2.54 mm</description>
</package>
</packages>
</library>
<library name="adafruit">
<packages>
<package name="0204/7">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
type 0204, grid 7.5 mm</description>
</package>
<package name="ARDUINOMICRO">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="IC1" library="linear" package="TO220H" value="7805T"/>
<element name="J1" library="SparkFun-Connectors" package="2X20_SHROUDED" value="RASPBERRYPI-40-PIN-GPIO_PTH">
<attribute name="PROD_ID" value="CONN-12263"/>
<attribute name="SF_ID" value="PRT-13054"/>
</element>
<element name="JP1" library="pinhead" package="1X02" value=""/>
<element name="LED_STRIP" library="pinhead" package="1X04" value=""/>
<element name="Q1" library="transistor-power" package="TO220BH" value="IRF1404"/>
<element name="Q2" library="transistor-power" package="TO220BH" value="IRF1404"/>
<element name="Q3" library="transistor-power" package="TO220BH" value="IRF1404"/>
<element name="R1" library="adafruit" package="0204/7" value="240"/>
<element name="R2" library="adafruit" package="0204/7" value="240"/>
<element name="R3" library="adafruit" package="0204/7" value="240"/>
<element name="U$1" library="adafruit" package="ARDUINOMICRO" value="ARDUINOMICRO"/>
</elements>
<signals>
<signal name="3.3V">
<contactref element="J1" pad="1"/>
<contactref element="J1" pad="17"/>
</signal>
<signal name="GND">
<contactref element="J1" pad="9"/>
<contactref element="J1" pad="25"/>
<contactref element="J1" pad="20"/>
<contactref element="J1" pad="14"/>
<contactref element="J1" pad="30"/>
<contactref element="J1" pad="34"/>
<contactref element="J1" pad="39"/>
<contactref element="Q1" pad="S"/>
<contactref element="Q2" pad="S"/>
<contactref element="Q3" pad="S"/>
<contactref element="LED_STRIP" pad="4"/>
<contactref element="U$1" pad="P$21"/>
<contactref element="J1" pad="6"/>
<contactref element="IC1" pad="2"/>
<contactref element="JP1" pad="1"/>
</signal>
<signal name="5V">
<contactref element="J1" pad="4"/>
<contactref element="J1" pad="2"/>
<contactref element="U$1" pad="P$20"/>
<contactref element="IC1" pad="3"/>
</signal>
<signal name="N$3">
<contactref element="Q1" pad="D"/>
<contactref element="LED_STRIP" pad="1"/>
</signal>
<signal name="N$1">
<contactref element="LED_STRIP" pad="2"/>
<contactref element="Q2" pad="D"/>
</signal>
<signal name="N$2">
<contactref element="LED_STRIP" pad="3"/>
<contactref element="Q3" pad="D"/>
</signal>
<signal name="R">
<contactref element="U$1" pad="P$2"/>
<contactref element="R1" pad="1"/>
</signal>
<signal name="G">
<contactref element="U$1" pad="P$3"/>
<contactref element="R2" pad="1"/>
</signal>
<signal name="B">
<contactref element="U$1" pad="P$4"/>
<contactref element="R3" pad="1"/>
</signal>
<signal name="SCL">
<contactref element="J1" pad="5"/>
<contactref element="U$1" pad="P$26"/>
</signal>
<signal name="SDA">
<contactref element="J1" pad="3"/>
<contactref element="U$1" pad="P$27"/>
</signal>
<signal name="12V">
<contactref element="IC1" pad="1"/>
<contactref element="JP1" pad="2"/>
</signal>
<signal name="N$4">
<contactref element="Q1" pad="G"/>
<contactref element="R1" pad="2"/>
</signal>
<signal name="N$5">
<contactref element="R2" pad="2"/>
<contactref element="Q2" pad="G"/>
</signal>
<signal name="N$6">
<contactref element="R3" pad="2"/>
<contactref element="Q3" pad="G"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
