Arduino

Guide

Tutorials

Reference

Hardware

Software

Blog

Forum

Playground

Exhibition

Hacking

FAQ

Buy

Reference Language (extended) | Libraries | Comparison

# Arduino Reference

See the extended reference for more advanced features of the Arduino languages.

Arduino programs can be divided in three main parts: structure, values (variables and constants), and functions. The Arduino language is based on C/C++.

## Structure An Arduino program run in two parts: void setup() void loop() setup() is preparation, and loop() is execution. In the setup section, always at the top of your program, you would set pinModes, initialize serial communication, etc. The loop section is the code to be executed -- reading inputs, triggering outputs, etc. Variable Declaration Function Declaration void #### Control Structures if if...else for switch case while do... while break continue return #### Further Syntax ; (semicolon) {} (curly braces) // (single line comment) /* */ (multi-line comment) #### Arithmetic Operators plus (addition) - (subtraction) * (multiplication) / (division) % (modulo) #### Comparison Operators == (equal to) != (not equal to) < (less than) > (greater than) <= (less than or equal to) >= (greater than or equal to) #### Boolean Operators && (and) || (or) ! (not) #### Compound Operators ++ (increment) -- (decrement) += (compound addition) -= (compound subtraction) *= (compound multiplication) /= (compound division) ## Variables Variables are expressions that you can use in programs to store values, such as a sensor reading from an analog pin. #### Constants Constants are particular values with specific meanings. HIGH | LOW INPUT | OUTPUT Integer Constants #### Data Types Variables can have various types, which are described below. boolean char byte int unsigned int long unsigned long float double string array ## Reference ASCII chart | ## Functions Digital I/O pinMode(pin, mode) digitalWrite(pin, value) int digitalRead(pin) Analog I/O int analogRead(pin) analogWrite(pin, value) - PWM Advanced I/O shiftOut(dataPin, clockPin, bitOrder, value) unsigned long pulseIn(pin, value) Time unsigned long millis() delay(ms) delayMicroseconds(us) Math min(x, y) max(x, y) abs(x) constrain(x, a, b) Random Numbers randomSeed(seed) long random(max) long random(min, max) Serial Communication Used for communication between the Arduino board and a computer or other devices. This communication happens via the Arduino board's serial or USB connection and on digital pins 0 (RX) and 1 (TX). Thus, if you use these functions, you cannot also use pins 0 and 1 for digital i/o. Serial.begin(speed) int Serial.available() int Serial.read() Serial.flush() Serial.print(data) Serial.println(data) Didn't find something? Check the extended reference.

Reference Home

Corrections, suggestions, and new documentation should be posted to the Forum.

The text of the Arduino reference is licensed under a Creative Commons Attribution-ShareAlike 3.0 License. Code samples in the reference are released into the public domain.

Edit Page | Page History | Printable View | Recent Site Changes