Arduino

Reference Language | Libraries | Comparison | Changes

## compound bitwise AND (&=)

#### Description

The compound bitwise AND operator (&=) is often used with a variable and a constant to force particular bits in a variable to the LOW state (to 0). This is often referred to in programming guides as "clearing" or "resetting" bits.

#### Syntax:

    x &= y;   // equivalent to x = x & y;

#### Parameters

x: a char, int or long variable
y: an integer constant or char, int, or long

#### Example:

First, a review of the Bitwise AND (&) operator

       0  0  1  1    operand1
       0  1  0  1    operand2
       ----------
       0  0  0  1    (operand1 & operand2) - returned result

Bits that are "bitwise ANDed" with 0 are cleared to 0 so, if myByte is a byte variable,
`myByte & B00000000 = 0;`

Bits that are "bitwise ANDed" with 1 are unchanged so,
`myByte & B11111111 = myByte;`

Note: because we are dealing with bits in a bitwise operator - it is convenient to use the binary formatter with constants. The numbers are still the same value in other representations, they are just not as easy to understand. Also, B00000000 is shown for clarity, but zero in any number format is zero (hmmm something philosophical there?)

Consequently - to clear (set to zero) bits 0 & 1 of a variable, while leaving the rest of the variable unchanged, use the compound bitwise AND operator (&=) with the constant B11111100

       1  0  1  0  1  0  1  0    variable
       1  1  1  1  1  1  0  0    mask
       ----------------------
       1  0  1  0  1  0  0  0

     variable unchanged
                         bits cleared

Here is the same representation with the variable's bits replaced with the symbol x

       x  x  x  x  x  x  x  x    variable
       1  1  1  1  1  1  0  0    mask
       ----------------------
       x  x  x  x  x  x  0  0

     variable unchanged
                         bits cleared

So if:

    myByte =  10101010;

    myByte &= B1111100 == B10101000;

See Also

- |= (compound bitwise or)
- & (bitwise AND)
- | (bitwise OR)

Reference Home

Corrections, suggestions, and new documentation should be posted to the Forum.

The text of the Arduino reference is licensed under a Creative Commons Attribution-ShareAlike 3.0 License. Code samples in the reference are released into the public domain.

Share|
©Arduino | Edit Page | Page History | Printable View | All Recent Site Changes