Next: H8/300 Opcodes, Previous: H8/300 Floating Point, Up: H8/300-Dependent

#### 9.10.4 H8/300 Machine Directives

`as` has the following machine-dependent directives for the H8/300:

`.h8300h`
  Recognize and emit additional instructions for the H8/300H variant, and also make `.int` emit 32-bit numbers rather than the usual (16-bit) for the H8/300 family.
`.h8300s`
  Recognize and emit additional instructions for the H8S variant, and also make `.int` emit 32-bit numbers rather than the usual (16-bit) for the H8/300 family.
`.h8300hn`
  Recognize and emit additional instructions for the H8/300H variant in normal mode, and also make `.int` emit 32-bit numbers rather than the usual (16-bit) for the H8/300 family.
`.h8300sn`
  Recognize and emit additional instructions for the H8S variant in normal mode, and also make `.int` emit 32-bit numbers rather than the usual (16-bit) for the H8/300 family.

On the H8/300 family (including the H8/300H) .word directives generate 16-bit numbers.