Arduino

Reference Language | Libraries | Comparison | Changes

## analogRead()

#### Description

Reads the value from the specified analog pin. The Arduino board contains a 6 channel (8 channels on the Mini and Nano, 16 on the Mega), 10-bit analog to digital converter. This means that it will map input voltages between 0 and 5 volts into integer values between 0 and 1023. This yields a resolution between readings of: 5 volts / 1024 units or, .0049 volts (4.9 mV) per unit. The input range and resolution can be changed using analogReference().

It takes about 100 microseconds (0.0001 s) to read an analog input, so the maximum reading rate is about 10,000 times a second.

#### Syntax

analogRead(pin)

#### Parameters

pin: the number of the analog input pin to read from (0 to 5 on most boards, 0 to 7 on the Mini and Nano, 0 to 15 on the Mega)

#### Returns

int (0 to 1023)

#### Note

If the analog input pin is not connected to anything, the value returned by analogRead() will fluctuate based on a number of factors (e.g. the values of the other analog inputs, how close your hand is to the board, etc.).

#### Example

    int analogPin = 3;     // potentiometer wiper (middle terminal) connected to analog pin 3
                           // outside leads to ground and +5V
    int val = 0;           // variable to store the value read

    void setup()
    {
      Serial.begin(9600);          //  setup serial
    }

    void loop()
    {
      val = analogRead(analogPin);    // read the input pin
      Serial.println(val);             // debug value
    }

#### See also

- analogReference()
- Tutorial: Analog Input Pins

Reference Home

Corrections, suggestions, and new documentation should be posted to the Forum.

The text of the Arduino reference is licensed under a Creative Commons Attribution-ShareAlike 3.0 License. Code samples in the reference are released into the public domain.

Share|
©Arduino | Edit Page | Page History | Printable View | All Recent Site Changes