<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.4">
<drawing>
<board>
<plain>
<wire x1="16.764" y1="-1.27" x2="95.174" y2="-1.27" width="0" layer="20"/>
<wire x1="95.174" y1="-1.27" x2="95.174" y2="53.584" width="0" layer="20"/>
<wire x1="95.174" y1="53.584" x2="16.764" y2="53.584" width="0" layer="20"/>
<wire x1="16.764" y1="53.584" x2="16.764" y2="-1.27" width="0" layer="20"/>
<text>JanW</text>
<text>2013</text>
<text>'Analog' like button</text>
<text>(J^3)</text>
</plain>
<libraries>
<library name="avr-6">
<description>&lt;b&gt;AVR Devices&lt;/b&gt;&lt;p&gt;
Version 5 - November 25, 2008.&lt;br&gt;&lt;br&gt;
Added ATmega164P/324P/644P devices for DIP and TQFP.
&lt;p&gt;
Version 4 - March 11, 2008.&lt;br&gt;&lt;br&gt;
This library now includes ONLY ATMEL AVR microcontrollers.  It is the result of merging all other available device libraries available at http://www.cadsoft.de/download as of the time it was made.  In addition to the legacy AT90* devices, it includes most ATMEGA devices including the new 48/88/168, most ATTiny devices and a set of ISP and JTAG pin headers.&lt;p&gt;
Based on the following sources:&lt;p&gt;
&lt;ul&gt;
&lt;li&gt;www.atmel.com
&lt;li&gt; file at90smcu_v400.zip
&lt;li&gt;avr.lbr and atmel.lbr as provided by CadSoft
&lt;li&gt;avr-1.lbr by David Blundell
&lt;li&gt;avr-2.lbr by Boris Zalokar
&lt;li&gt;avr-3.lbr by Carson Reynolds
&lt;li&gt;attiny24_44_84.lbr by Pawel Szramowski (ATTiny24/44/84 devices)
&lt;li&gt;atmel.lbr by Bob Starr (ISP headers)
&lt;li&gt;moates_custom_parts.lbr (edge ISP)
&lt;li&gt;other misc sources
&lt;/ul&gt;
&lt;author&gt;Revised by David Blundell (blundar at gmail dot com) and others.&lt;/author&gt;
&lt;p&gt;
&lt;author&gt;Added Mega162, Tiny2313 John Lussmyer (cougar at casadelgato.com)&lt;/author&gt;</description>
<packages>
<package name="DIL20">
<description>&lt;B&gt;Dual In Line&lt;/B&gt;</description>
</package>
</packages>
</library>
<library name="texas">
<description>&lt;b&gt;Texas Instruments Devices&lt;/b&gt;&lt;p&gt;
 &lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="DIL16">
<description>&lt;b&gt;Dual In Line Package&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="pinhead">
<description>&lt;b&gt;Pin Header Connectors&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="1X13">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
<package name="1X02">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="linear">
<description>&lt;b&gt;Linear Devices&lt;/b&gt;&lt;p&gt;
Operational amplifiers,  comparators, voltage regulators, ADCs, DACs, etc.&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="TO252">
<description>&lt;b&gt;SMALL OUTLINE TRANSISTOR&lt;/b&gt;&lt;p&gt;
TS-003</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="U$1" library="avr-6" package="DIL20" value="TINY2313-*P*"/>
<element name="IC1" library="texas" package="DIL16" value="L293E">
<attribute name="OC_NEWARK" value="89K0732"/>
<attribute name="MPN" value="L293E"/>
<attribute name="MF" value="Arrow Electronics"/>
<attribute name="OC_FARNELL" value="1467711"/>
</element>
<element name="IC2" library="texas" package="DIL16" value="L293E">
<attribute name="OC_NEWARK" value="89K0732"/>
<attribute name="MPN" value="L293E"/>
<attribute name="MF" value="Arrow Electronics"/>
<attribute name="OC_FARNELL" value="1467711"/>
</element>
<element name="IC3" library="texas" package="DIL16" value="L293E">
<attribute name="OC_NEWARK" value="89K0732"/>
<attribute name="MPN" value="L293E"/>
<attribute name="MF" value="Arrow Electronics"/>
<attribute name="OC_FARNELL" value="1467711"/>
</element>
<element name="JP1" library="pinhead" package="1X13" value=""/>
<element name="JP2" library="pinhead" package="1X02" value=""/>
<element name="JP3" library="pinhead" package="1X02" value=""/>
<element name="IC4" library="linear" package="TO252" value="7805DT"/>
</elements>
<signals>
<signal name="N$1">
<contactref element="JP1" pad="1"/>
<contactref element="IC1" pad="3"/>
</signal>
<signal name="N$2">
<contactref element="IC1" pad="6"/>
<contactref element="JP1" pad="2"/>
</signal>
<signal name="N$3">
<contactref element="IC1" pad="11"/>
<contactref element="JP1" pad="3"/>
</signal>
<signal name="N$4">
<contactref element="IC1" pad="14"/>
<contactref element="JP1" pad="4"/>
</signal>
<signal name="N$5">
<contactref element="IC2" pad="6"/>
<contactref element="JP1" pad="5"/>
</signal>
<signal name="N$6">
<contactref element="IC2" pad="11"/>
<contactref element="JP1" pad="6"/>
</signal>
<signal name="N$7">
<contactref element="IC2" pad="3"/>
<contactref element="JP1" pad="7"/>
</signal>
<signal name="N$8">
<contactref element="IC2" pad="14"/>
<contactref element="JP1" pad="8"/>
</signal>
<signal name="N$9">
<contactref element="IC3" pad="6"/>
<contactref element="JP1" pad="9"/>
</signal>
<signal name="N$10">
<contactref element="IC3" pad="11"/>
<contactref element="JP1" pad="10"/>
</signal>
<signal name="N$11">
<contactref element="IC3" pad="3"/>
<contactref element="JP1" pad="12"/>
</signal>
<signal name="N$12">
<contactref element="IC3" pad="14"/>
<contactref element="JP1" pad="13"/>
</signal>
<signal name="+5V">
<contactref element="IC3" pad="1"/>
<contactref element="IC3" pad="16"/>
<contactref element="IC3" pad="9"/>
<contactref element="IC2" pad="1"/>
<contactref element="IC2" pad="16"/>
<contactref element="IC1" pad="1"/>
<contactref element="IC1" pad="16"/>
<contactref element="IC1" pad="9"/>
<contactref element="IC2" pad="9"/>
<contactref element="U$1" pad="20"/>
<contactref element="IC4" pad="2"/>
</signal>
<signal name="+12V">
<contactref element="IC3" pad="8"/>
<contactref element="IC2" pad="8"/>
<contactref element="IC1" pad="8"/>
<contactref element="JP3" pad="2"/>
<contactref element="IC4" pad="1"/>
</signal>
<signal name="GND">
<contactref element="IC3" pad="4"/>
<contactref element="IC3" pad="5"/>
<contactref element="IC2" pad="4"/>
<contactref element="IC2" pad="5"/>
<contactref element="IC1" pad="4"/>
<contactref element="IC1" pad="5"/>
<contactref element="IC1" pad="13"/>
<contactref element="IC1" pad="12"/>
<contactref element="IC2" pad="13"/>
<contactref element="IC2" pad="12"/>
<contactref element="IC3" pad="13"/>
<contactref element="IC3" pad="12"/>
<contactref element="U$1" pad="10"/>
<contactref element="JP2" pad="2"/>
<contactref element="JP3" pad="1"/>
<contactref element="IC4" pad="3"/>
</signal>
<signal name="N$21">
<contactref element="U$1" pad="19"/>
<contactref element="IC2" pad="7"/>
</signal>
<signal name="N$22">
<contactref element="U$1" pad="18"/>
<contactref element="IC2" pad="15"/>
</signal>
<signal name="N$23">
<contactref element="U$1" pad="17"/>
<contactref element="IC2" pad="2"/>
</signal>
<signal name="N$24">
<contactref element="U$1" pad="16"/>
<contactref element="IC2" pad="10"/>
</signal>
<signal name="N$25">
<contactref element="U$1" pad="15"/>
<contactref element="IC3" pad="7"/>
</signal>
<signal name="N$26">
<contactref element="U$1" pad="14"/>
<contactref element="IC3" pad="15"/>
</signal>
<signal name="N$27">
<contactref element="U$1" pad="13"/>
<contactref element="IC3" pad="2"/>
</signal>
<signal name="N$13">
<contactref element="U$1" pad="12"/>
<contactref element="IC3" pad="10"/>
</signal>
<signal name="N$14">
<contactref element="U$1" pad="11"/>
<contactref element="IC1" pad="2"/>
</signal>
<signal name="N$15">
<contactref element="U$1" pad="9"/>
<contactref element="IC1" pad="7"/>
</signal>
<signal name="N$16">
<contactref element="U$1" pad="8"/>
<contactref element="IC1" pad="15"/>
</signal>
<signal name="N$17">
<contactref element="U$1" pad="7"/>
<contactref element="IC1" pad="10"/>
</signal>
<signal name="N$18">
<contactref element="U$1" pad="6"/>
<contactref element="JP2" pad="1"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
